SECTION 09 84 13 – FIXED SOUND-ABSORPTIVE PANELS

GENERAL

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes for wall panels.

Samples: [Selection samples.] [Verification samples.]

Informational Submittals:

Certificate of Compliance: Certification that installed products meet specified fire hazard requirements.

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by Madrid, Inc., [www.Madridinc.com](http://www.madridinc.com/).

Substitutions: [Refer to Division 01.] [Not permitted.]

MANUFACTURED UNITS

Fixed Sound-Absorptive Panel:

Product: CRETELight Absorb.

Backing: Honeycomb core.

Face: Micro-perforated, 0.6mm diameter.

Color: [Classic Grey.] [Classic White.] [Retro.] [to be selected from manufacturer’s full color range.]

Panel size: [48 inches wide x 118.9 inches long.] [Custom.]

Thickness: 3.4 inch.

Noise reduction coefficient: Minimum 0.90 tested to ASTM C423.

Edge Banding: [Matching panel] [No banding] [Beveled.] [Square.]

Weight: 2.4 pounds per square foot.

* 1. ACCESSORIES
     1. Mineral Wool: Manufacturers recommended material at not less than 2-inches.
     2. Attachment: Manufacturer recommended type.

EXECUTION

INSTALLATION

Install panels in accordance with manufacturer's instructions and approved Shop Drawings.

END OF SECTION