SECTION 09 84 13 – FIXED SOUND-ABSORPTIVE PANELS

 GENERAL

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes for wall panels.

 Samples: [Selection samples.] [Verification samples.]

 Informational Submittals:

 Certificate of Compliance: Certification that installed products meet specified fire hazard requirements.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by Madrid, Inc., [www.Madridinc.com](http://www.madridinc.com/).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MANUFACTURED UNITS

 Fixed Sound-Absorptive Panel:

 Product: CRETELight Absorb.

 Backing: Honeycomb core.

 Face: Micro-perforated, 0.6mm diameter.

 Color: [Classic Grey.] [Classic White.] [Retro.] [to be selected from manufacturer’s full color range.]

 Panel size: [48 inches wide x 118.9 inches long.] [Custom.]

 Thickness: 3.4 inch.

 Noise reduction coefficient: Minimum 0.90 tested to ASTM C423.

 Edge Banding: [Matching panel] [No banding] [Beveled.] [Square.]

 Weight: 2.4 pounds per square foot.

* 1. ACCESSORIES
		1. Mineral Wool: Manufacturers recommended material at not less than 2-inches.
		2. Attachment: Manufacturer recommended type.

 EXECUTION

 INSTALLATION

 Install panels in accordance with manufacturer's instructions and approved Shop Drawings.

END OF SECTION